**SPECIFICATION SHEET**

This is a Base Bid and the price may be increased or decreased. This bidder from whom petroleum products are being purchased shall provide written notice to the County of any change in price at least five (5) business days in advance. Upon receipt of written notice, Montgomery County shall request current price quotes in writing from all responsible and responsive offers. Montgomery County will record all bids, the petroleum product will be purchased from the most responsible, and responsive offers, taking into account the price change of the current supplier and the price quotes of the offers. Bids should be sealed and delivered to the Montgomery County Government Center, 1580 Constitution Row Ste A, Crawfordsville IN 47933.

All bids must be made upon Revised (1987) Form No. 95 (prescribed by the State Board of Accounts), which with the Forms of Proposal and Non-Collusion Affidavit attached thereto must be duly executed and sworn to. Bids must in all ways comply with the laws of the State of Indiana.

All bids returned must have a notarized Form NEP-3, Contractor's Nepotism Policy Compliance Affidavit.

All bids will be awarded to the most responsive and responsible bidder. The Montgomery County Board of Commissioners reserves the right to reject any and all bids if it determines it is in the County’s best interest to do so and to waive any informality in bidding.

Bidders shall make available to the County a confidential copy of the re trade price on the day of delivery to substantiate base price. Prices must be received by the County one day prior to delivery.

Montgomery County may test product delivered through an independent laboratory and will compare with specification submitted with bid. Any loads delivered which fail to meet specifications or certified standard analysis shall be removed and replaced by the supplier at no cost to Montgomery County.

Any portion of the bid, which will or may be subcontracted, shall be specified including the name of the subcontractor.

**EACH BIDDER MUST SPECIFY ON THE OUTSIDE OF THE ENVELOPE, WHICH ITEM IS BEING BID.**

**Gas, Fuel, Diesel Exhaust Fluid (DEF) and Oil Supplies**

|  |  |  |
| --- | --- | --- |
| **QUANTITY** | **DESCRIPTION** | **PRICE/GAL OR LB** |
| \*\*25,000 gallons or less | DIESEL, OFF ROAD |  |
| \*\*68,000 gallons or less | DIESEL, PREMIUM ON ROAD |  |
| \*\*500 gallons or less | NO LEAD GAS R+M/2 87.0 |  |
| 110 gallons or less | ISO 32 AW HYDRAULIC-Tote |  |
| 400 gallons or less | 15W 40 or EQUIVALENT-Tote |  |
| 240 lb. or less | PREMIUM GEAR OIL  80W90, 120 lb. drum |  |
| 275 gallons or less | HYDRAULIC OIL GRADE ISO  68AW, 55 gallon drum or bulk |  |
| 55 gallons or less | ANTI-FREEZE (Enviro Safe?) |  |
| 100 Gallons or less | Antifreeze Pure Fleet Red Heavy Duty or equivalent |  |
| 100 gallons or less | TRANSMISSION OIL DEXRON III/MERCON ATF  55 gallon drum or Tote |  |
| 330 gallons or less | UNIVERSAL TRACTOR HYDRAULIC/ WET BRAKE FLUID,  55 gallon drum or bulk |  |
| 4,000 gallons more or less | DEF – Diesel Exhaust Fluid  Purchase will be by the Tote |  |
|  |  |  |

ALL PRICES ABOVE DELIVERED TO HIGHWAY GARAGE

\*\* Bulk Transport or Tank Wagon Delivery as needed.

All Bidders must demonstrate capability to deliver the products when requested by the County Highway Department within a (24 hour time frame).

**PRICES QUOTED WITHOUT TAX**

|  |  |  |
| --- | --- | --- |
|  | OFF ROAD DIESEL | ON ROAD  PREMIUM DIESEL |
| API Gravity ASTM D-287 | 37-41 | Min 30 |
| Color (Typical) | Purple | Undyed |
| Copper Strip Corrosion ASTM D-130 (max) | 2 | 2 |
| Penskv-Martens Flash ASTM D-93 (min) | 125 | 125 |
| Sulfer ASTM D-4294 | 0.10 -0.15 | Max 0.05 |
| Viscosity 104 F ASTM D-445 |  |  |
| Pour Point ASTM D-97 | -20 to -30 | -20 to -30 |
| Calculated Cetane Index ASTM D-976 | 51 -55 | Min 45 |
| Diesel Index | 51 -55 | 45 -55 |
| Gross BTU/Gal (typical) | 136,000 | 138,000 |
| Distillation D-86 (typical) |  |  |
| IBP | 330 -360 | 330 - 360 |
| 10% | 370 -420 | 380 -420 |
| 50% | 455 -515 | 470 - 525 |
| 90% | 580 -670 | 540 - 640 |
| EBP | 630 -675 | 630 - 675 |

**PREMIUM UNLEADED**

|  |  |
| --- | --- |
| Motor Method (Min.)  (R + M /2 Octane (Min.) | N/A  87.0 |
| Lead Cone. (gm/gal) (Max.)  Lead Cone. (mm/gal) (Min.)  "ETHYL" MMT (gm/gal) (Min.) | 0.05  N/A  N/A |
| Sulfer Wt. % (Max.) | 0.04 |
| Oxidation Stability (Min.)  Existent Gum (mg/100) (Max.)  Conner Strip Corrosion (Max.) | 500  5  No. 1 |
| Additives:  Oxidation Inhibitor  Metal Deactivator  Multipurpose Additive  Dye | Present  Present  Present  Gold |

## EACH BIDDER MUST SPECIFY ON THE OUTSIDE OF THE ENVELOPE. WHICH ITEM IS BEING BID.